   Windows 98, Windows2000

   Introduction:
   -------------
   This document describes the procedure to install Windows 98
   and Windows 2000 driver for Realtek RTL8139 PCI Fast Ethernet adapter.

   Location of Driver:     \win98\RTL8139.SYS
                           \win2000\RTL8139.SYS

   Installing driver procedure on Microsoft Win98/windows2000 :
   -----------------------------------------------------
      1. When Windows 98/2000 is installed, please open " My Computer ", 
         and select " Control Panel " icon.

      2. Select " System " icon, and then select " Device Manager " page.

      3. Please remove " ?! PCI Ethernet Controller " device from " ?Other
         Devices " under device list with the " Remove " button.

      4. Please click on the Add New Hardware icon then click " Next " 
         button, click " Next " button one more times.

      5. This Wizard searches for new drivers for " PCI Ethernet 
         Controller ", you have to attempt to locate a driver provided
         by the manufacturer.

      6. Please insert the CD Driver into the CD drive, then click
         " Next " button.

      7. " What do you want Windows to do? ", Please click " search for
         the best driver for your device [Recommended] ", then click 
         " Next " button.

      8. Please click " Specify a location ", then type in 
         " D:\PIM-582\RT-8139A\WIN98 " or " D:\PIM-582\RT-8139A\WIN2000 ", then click
         " Next " button. The path depends on your Operation System.  
        Note: D: is the Drive where CD Driver has been inserted.

      9. The " Realtek RTL8139(A) PCI Fast Ethernet NIC " will be detected.
         Click " Next " button.

      10. Click " OK " to load netrts5.cat file.

      11. Please insert " Windows 98 CD-ROM " into the CD drive, then click
          " OK " button.
             
      12. Click " Finish " button to complete the installation and
          click " Yes " button to restart your system.
