   Windows 95 , OSR2.1

   Introduction:
   -------------
   This document describes the procedure to install  Windows 95 driver for
   Realtek RTL8139 PCI Fast Ethernet adapter.

   Location of Driver:     \WIN95\RTL8139.SYS

   Installing driver procedure on Microsoft Windows 95 :
   -----------------------------------------------------

      1. Excuting Windows 95 Setup. When " Analying your computer " dialog
         box is appeared, please click the check box to " Network Adapter".
         Then click [Next] to continue.
          
      2. When Windows 95 is installed. Please upgrade your Windows 95 to 
         OSR2.1 if your Windows 95 is older version. Please load 
         usbsupp.exe and winp2x4.exe files from \95_upgrd directory in the
         CD Driver disk.

      3. The Update Device Driver Wizard will detect the PCI Ethernet 
         Controller. You have to attempt to locate a CD Driver disk provided
         by the manufacturer.

      4. Please insert the CD Driver disk into the CD drive, then click
         " Next " button.

      5. Click " Other Locations... " button.

      6. type in X:\PIM-582\RT-8139A\WIN95 in the Location, then click on [OK]. 
         (X: is the drive where CD Driver disk has been inserted)

      7. Windows will found the Realtek RTL8139 PCI Fast Ethernet. Click
         " Finish " button.

      8. Please insert the " Windows 95 CD-ROM " into CD drive, then click
         " OK " button. Type in " X:\WIN95 ", then click " OK " button.
         (X: is the drive where CD Driver disk has been inserted)

      9. When system will load the netrts.inf file, please insert the CD Driver
         disk into CD drive, then type in X:\PIM-582\RT-8139A\WIN95.
         (X: is the drive where CD Driver disk has been inserted)

      10. Click " OK " button.


      11. You must provide computer and workgroup names then click on [Close].

      12. The " Copying Files " dialog box will be appeared. Please insert
          the " Windows 95 CD ROM " and click [OK].

      13. System will load the netapi.dll file. Type in " X:\WIN95 ", then
          click " OK " button.
         (X: is the drive where CD disk has been inserted)
       
      14.Click on [Yes] to complete the installation and restart your
         system.The RTL8139 PCI Fast Ethernet card will be detected.


                                                   
