These drivers are provided for convenience.  They are designed for
Unixware version 7.0.1 and later.  For any and all UNIX support questions
as well as updated drivers, please contact the OS vendor.

Installing the eeE Driver for UnixWare* 7 
========================================

To install the eeE driver for UnixWare 7:
     
1. Copy the eeE.pkg file into any directory on the 
   UnixWare system, such as in the /tmp directory.
     
2. Make sure no other users are logged on and all user applications
   are closed.
     
3. If there is an older version of the eeE driver on the system, first
   run 'netcfg' and remove any configured NICs. Exit 'netcfg'. 
   
4. Install the new driver using 'pkgadd'. For example:
     
        # pkgadd -d /tmp/eeE.pkg
     
5. Run 'netcfg' to add and configure the NICs. 

6. Reboot the system.
     
NOTE:  If you require Hot Plug PCI capabilities, the DDI 8 eeE driver must 
be used.  The DDI 8 driver is supported on UnixWare 7.1.0 and later 
versions.  For more information about Hot Plug PCI capabilities please 
refer to SCO UnixWare 7 documentation.

* Third-party trademarks are the property of their respective owners.
