   Intel's Advanced Networking Services for NetWare* 4.1x and Higher 

CONTENTS:
   I. INTRODUCTION
  II. REQUIREMENTS
       Switch capabilities
       Server Adapters Supported
 III. LOCATIONS of ANS DRIVER
  IV. TEAMING COMMAND LINES 
       Basic Structure
       Example Mixed Speed Fault Tolerance Team
   V. VLANS COMMAND LINES
       Allocating Memory for VLANs
       Example for a Single Adapter VLAN Team
  VI. USAGE NOTES
*   *   *   *   *   *   *   *   *   *    *   *   *   *   *   *   *

I. INTRODUCTION

  iANS.LAN is the Intel software for NetWare 4.11 and higher that 
  provides a variety of advanced networking services (ANS). These 
  benefits include the teaming and VLAN based features. 

  Teaming includes:

    Adapter Fault Tolerance (AFT),
    Adaptive Load Balancing (ALB), 
    Port Aggregation (Intel Link Aggregation, Cisco* Fast EtherChannel* (FEC)
                      or Gigabit EtherChannel* (GEC), 

  VLAN (Virtual LAN) support includes support of IEEE 802.1q and Cisco ISL*.

  With NetWare, VLAN and ANS (teaming) features may be used simultaneously.
  
  Descriptions of the various modes and their specific requirements are:

  AFT (Adapter Fault Tolerance). Default mode. A secondary adapter
  in the team will automatically take over on any failure 
  of the primary connection (cable, adapter or port). Only one
  card is active at a time. If there is a failover to a
  second card, control passes back to the primary adapter 
  when it is restored. May use a mixed speed team. May use a 
  hub or any switch.

  ALB (Adaptive Load Balancing or asymmetrical link aggregation).
  A team of 2-8 adapters share the transmission load while 
  the primary receives and transmits. Includes fault tolerance
  support. Should be a same speed team. May use any hub or 
  switch.    

  FEC (Cisco*'s Fast EtherChannel* Technology and Intel Link 
  Aggregation).  A team of 2-8 adapters which simultaneously
  receive and transmit. Includes fault tolerance support. 
  Should be a same-speed team. Requires a switch that supports
  Intel Link Aggregation or Cisco's FEC. Spanning Tree Protocol
  must be turned off.

  GEC - Gigibit equivalent of FEC. Requires GEC compatable switch and
  Gigabit Adapters.


  You may also identify which adapters in a team you want to use as the
  primary and secondary cards. The Primary will be the first card to be
  used in a team. For fault tolerance, the primary is the only card used
  until a failure. For ALB, the primary is the card that both transmits
  and receives. The Secondary is the preferred adapter (in a more than 2
  card team) to fill the role of primary adapter upon a failure of the
  primary.


  VLAN (Virtual LAN):
 
  VLANs will be enabled if a vlanID is stated when iANS is first loaded.
  VLAN is a network subset formed through software rather than hardware 
  proximity. VLANs provide secure access, segmented broadcast 
  traffic, and centralized management for improved performance. 
  Requires a VLAN capable switch (10 or 100). Connection must be made to
  ports tagged with numbers identical to that assigned to the adapter. 802.1q 
  support is provided by all Intel PRO/100 adapters except the PRO/100B. 
  Cisco ISL VLAN support is provided by the PRO/100 Intelligent Server 
  adapter. Additionally the PRO/100 Intelligent Server adapter provides 
  Cisco ISL VLAN support if on the Load iANS line you add "vlanmode=ISL". 
  There is a limit of 64 VLANs per server.


*   *   *   *   *   *   *   *   *   *    *   *   *   *   *   *   *
    
II. REQUIREMENTS:

  These advanced networking features only work with Intel Server adapters. 

  Each team requires at least one Server adapter.

  All adapters must use the same frame type parameter.
  
  Some features require a connection to a switch (preferably 100baseTX or
  greater) that has link aggregation and/or VLAN capability. 

  Link all adapters of an ALB, FEC or GEC team to the same segment using
  the same speed and duplex, otherwise performance will be greatly degraded.
  AFT teams must also be connected to the same segment but may consist of
  adapters using different speeds and duplex modes.  If using different speed
  adapters on an AFT team, set the fastest adapter as the "primary". 

  When using iANS.LAN, do NOT bind the network protocols (IPX, IP, etc)
  directly to the base driver of an adapter used with iANS. Instead, bind 
  iANS to the base driver and the protocol(s) to iANS.  Doing otherwise can
  cause routing error messages, but most likely the protocols bound directly
  to the base drivers will simply not work.

  The install utility (INSTALL.NLM for NetWare 4.x, and NWCONFIG.NLM for
  NetWare 5.0) should not be used to configure iANS.LAN because of the 
  configuration complexity of this driver.  It may be used to copy iANS.LAN
  into place which will be done automatically if the utility is used to 
  install CE100B.  However, an attempt to install and configure iANS.LAN with
  that tool will result in several lines being added to the AUTOEXEC.NCF that
  appear as a normal LAN driver load and bind statement.  These lines will need
  to be removed or replaced with a valid set of iANS commands.  An alternative
  is to manually copy the the iANS.LAN driver to the sys:\system directory.

  Some advanced features are also adapter dependent as the table below depicts.
  The term "Teaming' used here implies teaming modes of AFT(T), ALB(B), FEC(F),
  and GEC(G).

   Server Adapters supported              Teaming     VLAN(.1q)   VLAN(ISL)
                                          T B F G 
   PRO/1000 Gigabit Server Adapter        x x   x        x           
   PRO/100 Intelligent Server Adapter     x x x          x           x
   PRO/100+ Server Adapter                x x x          x           
   PRO/100+ Dual Port Server Adapter      x x x          x           
   PRO/100 and PRO/100 S Server Adapters  x x x          x       
    
   Note: Only fault tolerance should use mixed speed teams.      
   All other Intel PRO/100 adapters may be part of an ANS team with all 
   features except for some VLAN capability. All PRO/100 except the PRO/100B
   adapter will work for 802.1q VLAN. 

  For more information on features, switches, and specific adapter 
  compatability, see the Intel web site.


*   *   *   *   *   *   *   *   *   *    *   *   *   *   *   *   *

III. LOCATIONS of ANS DRIVER (required for some ANS features):
 
  For PRO/100+ Server Adapters:   
  \NWSERVER\iANS.LAN 

  For PRO/1000 and PRO/100 Intelligent Server Adapters:
  http://www.intel.com/support 

  (Navigate to "Software & Driver Downloads", "Network Products",
  "Ethernet Adapters", then to the appropriate adapter listing.)


*   *   *   *   *   *   *   *   *   *    *   *   *   *   *   *   *

IV. COMMAND LINES 

  Basic Structure:
  LOAD base driver (e.g. CE100B.LAN) with appropriate parameters.

  LOAD iANS driver 
     For a VLAN you would include a VLAN ID number.
     For a VLAN or multiple frame type configuration, include a name.
     For a multiple team setup include a team number.

  BIND iANS driver to adapter name.
     If creating multiple teams, include the team # here to define which 
      team uses which adapter(s).
     If you want to specify which adapter is to be primary or secondary,
      list on this line.

  LOAD iANS COMMIT <mode>. Creates the team. 
     (<Mode> will distinguish among AFT, ALB, FEC or GEC.)
     If creating multiple teams, include the team #.

  BIND the protocol to the iANS driver using the name that was assigned when
  iANS was loaded.
     If you are using only one frame type, a single team and no VLAN, you can
     bind the protocol directly to the iANS driver without using an assigned
     name. Include a net=n number (especially in a script since the system will
     request the number if not given.)

  Example of Mixed Speed Fault Tolerance Team:

  Load CE100b name=100Meg
  Load CE1000 name=Gigabit
  Load iANS
  Bind iANS Gigabit Primary
  Bind iANS 100Meg
  Load iANS COMMIT MODE = AFT
  Bind IPX iANS Net=2


  For more information on specific load commands for AFT, ALB or FEC 
  see the Adapter Teaming example file (examples.txt) in the 
  \Info\NetWare directory on the CD.


*   *   *   *   *   *   *   *   *   *    *   *   *   *   *   *   *

V. VLAN COMMAND LINES 

  Allocating Memory for VLANS:

   When using multiple VLANs, the server's default packet buffers will probably
   need to be increased.  To do this, add the following lines to the STARTUP.NCF
   file which is located in the same directory that NetWare is launched from.
   Usually C:\NWSERVER\STARTUP.NCF:

   SET MINIMUM PACKET RECEIVE BUFFERS = 200 (or higher)
   SET MAXIMUM PACKET RECEIVE BUFFERS = 500 (or higher)

   "SET MINIMUM PACKET" designates the minimum number of packet receive buffers
   the system will allocate and "SET MAXIMUM PACKET" designates the maximum.
   Make sure that the maximum setting is equal to or greater than the minimum
   setting.  The number of buffers required is based on the number of VLANs
   and whether or not load balancing or FEC / GEC is in use.

   For every VLAN used, iANS will request 64 buffers.  When in load sharing
   modes (ALB, FEC and GEC) 64 buffers are needed for each adapter in the team.
   The non load sharing fault tolerant mode (AFT) only requires the 64 buffers
   for one of the adapters in the team.

   As an example, an ALB team of 2 adapters that uses 12 VLANs would require
   64 [buffers] * 2 [adapters] * 12 [VLANs] = 1536 for the minimum packet 
   receive buffers.  This number is in addition to any other buffers that the 
   server may require for other purposes.

   The default amount of memory used by each NetWare receive buffer is 
   approximately 4K (varies slightly with different versions).  If the extra 
   memory requirement for VLAN is a problem, there are several things that can
   be done to reduce the impact.

   If ethernet is the only network topology that the server uses, the size of 
   the buffer can be reduced to 2000 bytes (the maximum ethernet frame size plus 
   some out of band data used by iANS) without impacting the performance of the 
   server.  This is done by adding the following line to the STARTUP.NCF file:

   SET MAXIMUM PHYSICAL RECEIVE PACKET SIZE = 2048

   Note that this will not work if ethernet "jumbo frames" are in use. In fact, 
   the packet size will have to be increased to accommodate the Jumbo Frames.
   Jumbo frames are supported only with the Gigabit adapter and requires switch 
   infrastructure that supports Jumbo Frames.

   A keyword is included for iANS that allows the administrator to reduce the 
   buffer requirement per VLAN from 64 down to as low as 32, however, this will
   negatively impact the server's performance.  The syntax is:

   LOAD IANS TX_ECBS_TO_USE = X

   Where "X" is the number of buffers to use for each VLAN.


  Example for a Single 802.1q VLAN Team:

   Load ce100b slot=5 frame=ethernet_802.3 name=e83
   Load ians vlanid=2 frame=ethernet_802.3 name=T1-VL2 team=1
   Load ians vlanid=3 frame=ethernet_802.3 name=T1-VL3 team=1
   Bind ians e83 team=1
   Load ians commit mode=AFT team=1
   Bind ipx T1-VL2 net=2
   Bind ipx T1-VL3 net=3)


  See examples.txt for several examples of configuring teams, vlans and both.


  In order to function properly, the adapters configured for VLAN must
  be connected to a "tagged" port (called a trunk port by Cisco) on an
  802.1q capable switch.


*   *   *   *   *   *   *   *   *   *    *   *   *   *   *   *   *

VI. USAGE NOTES:

  1. Gigabit adapters - The PRO/1000 adapter may be teamed with certain
     Intel(R) Fast Ethernet adapters for AFT mode only. The PRO/1000 should 
     be designated the preferred primary adapter for best performance.  
     Drivers may be found on the Intel web site.

     Intelligent Server Adapters (CE100snw basedriver) also require a
     recent basedriver (ce100snw v.1.20 or later), available on the Intel 
     web site.

  2. Required Settings in STARTUP.NCF   

      SET MINIMUM PACKET RECEIVE BUFFERS = 200 (or larger)
      SET MAXIMUM PACKET RECEIVE BUFFERS = 500 (or larger)

      See the section "Allocating Memory for VLANS" in Section V. VLAN
      COMMAND LINES earlier in this document for more information.

  3. If you receive the ERROR MESSAGE (at commit): "Failed to create new
     team," check the following:

   a. All adapters have loaded drivers and have the same frame types
      loaded. 

   b. iANS is loaded once for each vlan and frame type.

   c. All adapters are connected to the same network segment.

   d. iANS is not being bound to an unsupported adapter.

   e. An "iANS BIND" command has been issued for each adapter and
      frame type in the team.  

   Note: Novell's CONFIG command will not reflect the iANS BIND
   statements until after the COMMIT has been successfully issued.

  4. To display the current status for all adapters in a iANS team:
     LOAD iANS STATUS team=(name)

  5. To create the primary adapter: 
     BIND iANS <adapter> PRIMARY
     Example: BIND iANS CE100B_1_E82 PRIMARY
     This can only be done during in the BIND command.

  6. The default amount of memory used by each NetWare receive buffer 
     is approximately 4K (varies slightly with different versions).  
     If the extra memory requirement for VLAN is a problem, there are 
     several things that can be done to reduce the impact:

   a. If Ethernet is the only network topology that the server uses,
      and you are not using "jumbo frames", add (to STARTUP.ncf):

      SET MAXIMUM PHYSICAL RECEIVE PACKET SIZE = 2048
      
   b. Use the iANS keyword TX_ECBS_TO_USE to reduce the buffers per
      VLAN from 64 down to as low as 32. This WILL negatively impact
      performance (while reducing system resources required).  

      Example: LOAD IANS TX_ECBS_TO_USE = n (# buffers for each VLAN)

      See the section "Allocating Memory for VLANS" in Section V. VLAN
      COMMAND LINES earlier in this document for more information.


*  Third-party trademarks are the property of their respective owners.
