   Other Operating Systems

     Installation Notes for Intel(R) Server and Client Adapters in
     Other Operating Systems


CONTENTS
 - USING IBM LAN SUPPORT FOR AS/400 AND NETWARE
    o Installing and Configuring the Adapter
 - LAN SERVER INSTALLATION NOTES
    o General Installation - LAN Server and OS/2 Requester (4.0 or 3.0)
    o General Installation under DOS (DOS LAN Services)
    o General Installation under DOS: LAN Support Program (LSP)
    o General Installation under DOS (DOS LAN Requester)
 - BANYAN* NDIS WORKSTATION INSTALLATION NOTES
    o General Installation
    o Hints and Tips
 - LANTASTIC* 6.0 INSTALLATION NOTES
    o General Instructions and Sample Configuration Files
    o Hints and Tips
    o Sample Files
 - GENERAL NDIS 2.X DRIVER NOTES
    o Sample Configuration Files
    o General Notes
    o Hints and Tips
 - ADVANCED SETTINGS


     ***         ***         ***         ***          ***         ***


 - USING IBM LAN SUPPORT FOR AS/400 AND NETWARE
   ============================================

Installing and Configuring the Adapter
======================================

Location of Driver:  \DOS\E100B.DOS (for LANSUP)
Location of Driver:  \DOS\E100BODI.COM (for ODINSUP)


(Sample configuration files are included below.)


General instructions
--------------------

There are two ways to connect an Intel adapter simultaneously
to an IBM AS/400 (or other host based on DLC protocol) and
a Novell server:

- Using LANSUP.COM (NDIS-based) or
- Using ODINSUP.COM (ODI-based)

LANSUP.COM and ODINSUP.COM are Novell drivers included in VLMUPx.EXE
(where x is the number of the latest version). The files are available
on Novell's Support Web site.


Sample CONFIG.SYS file for LANSUP
---------------------------------

DEVICE = C:\LANMAN\PROTMAN.DOS    (version 1.1 or later )
DEVICE = C:\LANMAN\E100B.DOS      (version 1.34 or later)
DEVICE = C:\LANMAN\DXMA0MOD.SYS   (version 1.35 or later)
DEVICE = C:\LANMAN\DXME0MOD.SYS   (version 1.35 or later)
DEVICE = C:\PCS\EIMPCS.SYS
DEVICE = C:\PCS\ECYDDX.SYS


Sample AUTOEXEC.BAT file for LANSUP
-----------------------------------

CD\LANMAN
NETBIND                         (version 1.1 or later )
LSL                             (version 2.11 or later)
LANSUP                          (version 1.27 or later)
IPXODI                          (version 2.20 or later)
NETX or VLM                     (version 3.32 or later of
                                 NETX.EXE, or version 1.20
                                 or later of VLM.EXE)
F:
LOGIN
C:\PCS\STARTPCS


Sample PROTOCOL.INI file for LANSUP
-----------------------------------

[PROTOCOL MANAGER]
   DRIVERNAME = PROTMAN$

[ETHERNET]
   DRIVERNAME = DXME0$
   BINDINGS = E100B

[E100B]
   DRIVERNAME = E100B$


Sample NET.CFG file for LANSUP
------------------------------

Link Driver LANSUP
   Max Frame Size = 1490

NetWare DOS Requester
   First Network Drive = F


Sample CONFIG.SYS file for ODINSUP
----------------------------------

DEVICE = \LANMAN\PROTMAN.DOS /I:C:\LANMAN   (version 1.1 or later)
DEVICE = \LANMAN\DXMA0MOD.SYS              (version 1.35 or later)
DEVICE = \LANMAN\DXME0MOD.SYS              (version 1.35 or later)
DEVICE = C:\PCS\EIMPCS.SYS
DEVICE = C:\PCS\ECYDDX.SYS


Sample AUTOEXEC.BAT file for ODINSUP
------------------------------------

CD\LANMAN
LSL                                       (version 2.11 or later)
E100BODI                                  (version 1.25 or later)
ODINSUP                                   (version 2.00 or later)
NETBIND                                   (version 1.1 or later)
IPXODI                                    (version 2.20 or later)
NETX or VLM                    (version 3.32 or later of NETX.EXE;
                                version 1.20 or later of VLM.EXE)
F:
LOGIN
C:\PCS\STARTPCS


Sample PROTOCOL.INI file for ODINSUP
------------------------------------

[PROTOCOL MANAGER]
   DRIVERNAME = PROTMAN$

[ETHERNET]
   DRIVERNAME = DXME0$
   BINDINGS = E100BODI

[E100BODI]
   DRIVERNAME = E100BODI$


Sample NET.CFG (C:\LANMAN\NET.CFG) file for ODINSUP
---------------------------------------------------

Link Driver E100BODI
   Frame ethernet_802.2
   Frame ethernet_II
   Frame ethernet_802.2
   Frame ethernet_snap

Protocol ODINSUP
   Bind  E100BODI

NetWare DOS Requester
   First Network Drive = F


     ***         ***         ***         ***          ***         ***


 - LAN SERVER INSTALLATION NOTES
   =============================

Location of files:  \OS2\E100B.OS2   (OS/2* driver)
                    \OS2\E100BEO2.NIF
      
                         or
      
                    \DOS\E100B.DOS   (DOS driver)
                    \DOS\E100BEDS.NIF (DLR and LSP installation file)

NOTE: LAN Requester needs DOS 3.3 through 5, but if you're using DOS 6.0
      or higher, run SETVER.EXE prior to using the executable files 
      found on the DOS LAN Requester disks. See your DOS manual if you
      need help with SETVER.EXE.


Sample Configuration File
-------------------------

PROTOCOL.INI (will include):

[E100B_NIF]
   DriverName = E100B$


General Installation - LAN Server and OS/2 Requester (4.0 or 3.0)
-----------------------------------------------------------------

1  Run the MPTS utility with LAN Server 4.0 or OS/2 Requester 4.0 (Run
   the LAPS utility with LAN Server 3.0 or OS/2 Requester 3.0).

2  Click Install.

3  When prompted, insert the Configuration and Drivers disk in the
   drive, specify <drive>:\OS2 for driver location, and click OK.

4  When Install reads the E100BEO2.NIF, installation is complete. Click
   OK.  The adapter driver has been copied to your system.

5  Click Configure from the MPTS window.

6  At the Configure window, make sure the LAN adapters and protocols
   button is on and click CONFIGURE.

7  At the LAPS Configuration window, select the Intel adapter (OS/2
   driver: E100B.OS2) from the Network Adapters window.
   
   Click Add in the Network Adapter window to add the Intel PCI
   adapter to the current configuration.

8  Select your desired protocol(s) from the Protocol window and click
   Add to add the protocol(s) to the current configuration.

9  Click OK when you're done and follow the prompts to exit MPTS. Your
   CONFIG.SYS is automatically updated.
   
   Shut down and reset your system for the changes to take effect.


General Installation under DOS (DOS LAN Services)
-------------------------------------------------

NOTE: Due to a problem with the DLS installation utility, you need to
      complete the following steps before executing the installation of
      DLS:
   
      1  On DLS Diskette 1, make a directory off the root called NDIS.
      
      2  Copy the file E100B.DOS (from the \DOS directory of the
         Configuration and Drivers disk) into this new directory \DOS
         on DLS disk 1.

1  Run the DOS LAN Services installation program at the DOS workstation.
   Follow the prompts.

2  When presented with an adapter list, select Network card not shown in
   list below.

3  When prompted for the location of the OEMSETUP.INF file, insert the
   Configuration and Drivers disk in your drive and enter <drive>:\DOS
   as the path.

4  Select the Intel adapter from the list.  Follow the prompts.

5  Enter your machine name, user name and domain name.

6  Set the options as you need; then highlight "The listed options are
   correct" and press Enter.

7  Accept the defaults on the next screen, highlight "The listed options
   are correct" and press Enter.

8  Set the Speed, Duplex mode, or Slot Device if needed. We recommend
   accepting the defaults. Then highlight "The listed options are
   correct" and press Enter.

9  You may be asked to insert DLS disks. Follow the prompts to complete
   the installation and restart your computer for changes to take 
   effect.


General Installation under DOS - LAN Support Program (LSP)
---------------------------------------------------------

1  Run DXMAID from the LAN Support Program disk.

2  Follow the prompts and instructions.

3  When prompted, insert the Configuration and Drivers disk and
   enter the pathname <drive>:\DOS.

4  The default configuration is suitable for most environments.  We
   recommend accepting the defaults.

5  After the installation is complete, restart your computer for the
   changes to take effect.


General Installation under DOS - (DOS LAN Requester)
----------------------------------------------------

1  Run the DOS LAN Requester installation program at the DOS
   workstation. Follow the prompts to configure your DOS LAN Requester
   as you require.

2  After the installation is complete, restart your computer for the
   changes to take effect.


Advanced Settings for PROTOCOL.INI
----------------------------------
See the Advanced Settings section.

     ***         ***         ***         ***          ***         ***


 - BANYAN* NDIS WORKSTATION INSTALLATION NOTES
   ===========================================

Location of Driver:  \DOS\E100B.DOS


Sample Configuration Files
--------------------------

CONFIG.SYS (will contain):
   
   DEVICE=C:\BAN\PROTMAN.DOS /I:C:\BAN
   DEVICE=C:\BAN\E100B.DOS

PROTOCOL.INI:
   
   [E100B_NIF]
      Drivername = E100B$


General Installation
--------------------

1  The Intel adapter uses an NDIS 2.0.1 driver to connect
   to a Banyan server. If you have an NDIS client disk prepared, skip to
   step #6.

2  To create an NDIS client disk, run PCCOPY (located on the Z drive of
   the Banyan server).

3  Choose PC Configuration Software and/or LAN driver, then select NDIS
   Ethernet and PCCONFIG.

4  Choose the appropriate DOS redirector. For example, REDIRALL for all
   versions of DOS.

5  Specify the directory you want the client software copied to. The
   default is A:\.

6  On the client you're setting up, copy the NDIS client software to a
   directory on the hard drive.

7  Run Banyan's PCCONFIG program.

8  Select Network Card Settings and page down to select the NDIS
   Ethernet option.

9  Specify E100B_NIF as the PROTOCOL.INI bindings parameter.

10 Select Login Environment Settings, then select Default Communications
   Driver. Page down to select the NDIS Ethernet option.

11 Save the settings and exit PCCONFIG.

12 Copy the PROTOCOL.INI and E100B.DOS files located in the NDIS
   subdirectory on the Configuration and Driver disk to the BAN
   subdirectory or other directory where Banyan client files are
   located. Modify the PROTOCOL.INI file to make sure the file contains
   the line [E100B_NIF] above the DRIVERNAME=E100B$ line.

13 Add the lines to your CONFIG.SYS file as shown in the Sample
   Configuration Files section above.

14 Reboot and run BAN to attach to the Banyan server.


Hints and Tips
--------------

1  Error Message with PRO0025E:

   This type of message occurs when the driver attempts to bind to the
   protocol manager. It usually indicates there's a syntax or other
   error in the PROTOCOL.INI file. Review the file carefully for errors.
   Also, verify parameters entered in PCCONFIG. For additional
   information, see NDISBAN.DOC which is part of the NDIS Banyan client
   software.

2  Make sure your NDISBAN.COM is dated April 1994 or later. Earlier
   versions may not work properly.

3  Parameters for the PROTOCOL.INI file are in the Advanced Settings
   section.


     ***         ***         ***         ***          ***         ***


 - LANTASTIC* 6.0 INSTALLATION NOTES
   =================================

Location of driver:     \DOS\E100B.DOS

General Instructions and Sample Configuration Files
---------------------------------------------------

The installation procedure transfers files to a specific directory on
the workstation and creates or modifies existing configuration files to
fit your specific needs.  The installation utility, INSTALL.EXE, is
located on LANtastic Network Software Disk 1.

1  Run INSTALL.EXE from Disk 1.

2  The LANtastic Install program screen appears. You must complete each
   of the questions. These options are specific to your needs.
   
   1  Asks for a unique computer name.
   
   2  Asks you to select the drive that you want LANtastic to be
      installed on. The default is Drive C:.
   
   3  Asks you to specify a directory where you want the LANtastic files
      to be installed. The default is \LANTASTI.
   
   4  Asks if you want to share your computer's drives or printers.
   
   5  Asks you to select the maximum number of connected computers.
   
   6  Prompts you to select any other LANtastic features that you may
      want to install.
   
   7  Summarizes the options you selected. If it looks correct, continue
      with the installation.
   
   8  Prompts you to select a network adapter to run your LANtastic
      software on. From the list of adapters, select "NDIS SUPPORT FOR
      NETWORK ADAPTERS".
   
   9  Asks you to insert the manufacturer's driver diskette. Insert the
      adapter Configuration and Drivers diskette into the drive and
      specify the source path for driver files <drive>:\DOS.
   
   10 Asks if you want to Set Up Permanent Drive or Printer Connections.
   
   11 Summarizes the options you selected. If they are correct, choose
      Perform the Installation and LANtastic will install the files.


Hints and Tips
--------------

Below are sample CONFIG.SYS, STARTNET.BAT and PROTOCOL.INI files. These
are the three files with Intel adapter configuration options that
the install program creates. For details on PROTOCOL.INI parameters, see
the end of this document.


Sample CONFIG.SYS file
----------------------

DEVICE=C:\LANTASTI\PROTMAN.DOS /I:C:\LANTASTI
DEVICE=C:\LANTASTI\E100B.DOS
FILES=100
BUFFERS=30


Sample C:\LANTASTI\STARTNET.BAT file
------------------------------------

@echo off
rem LANtastic  Version 6.00  installed 95/12/04 03:38:23
rem (for Windows)
C:
cd C:\LANTASTI
SET LAN_CFG=C:\LANTASTI
rem If LANtastic is disabled, skip everything.
IF EXIST DISABLED GOTO :STARTNET_DONE

@echo ===== Begin LANtastic configuration =====
PATH C:\LANTASTI;C:\LANTASTI\NW;%PATH%
SET LAN_DIR=C:\LANTASTI.NET
SET NWDBPATH=C:\LANTASTI\NW
LOADHIGH AI-NDIS BIND_TO=E100B_NIF
AILANBIO @STARTNET.CFG
REDIR LAB1 @STARTNET.CFG
IF EXIST NOSHARE GOTO :NOSHARE
SERVER C:\LANTASTI.NET @STARTNET.CFG
NET LOGIN \\LAB1
GOTO :CONTINUE
:NOSHARE
@echo LANtastic server was installed but turned off.
:CONTINUE
rem If CONNECT.BAT exists, run it to set up connections.
IF EXIST CONNECT.BAT GOTO :CONNECT
rem Otherwise set up connections specified during install.
NET USE LPT1: \\LAB1\@PRINTER
NET LPT TIMEOUT 10
GOTO :CONNECT_DONE
:CONNECT
@echo Setting up LANtastic connections from CONNECT.BAT
rem Build CONNECT.BAT like this: "NET SHOW/BATCH >
C:\LANTASTI\CONNECT.BAT"

call CONNECT.BAT
:CONNECT_DONE
NET POSTBOX
@echo ===== End LANtastic configuration =====

:STARTNET_DONE
cd \


Sample C:\LANTASTI\PROTOCOL.INI file
------------------------------------

;PROTOCOL.INI for LANtastic Version 6.00

;--- using a Intel Adapter

[PROTMAN]
   DRIVERNAME = PROTMAN$
   DYNAMIC = YES

; PROTOCOL.INI section for the Intel Adapter.

[E100B_NIF]
   DRIVERNAME = E100B$

Parameters for the PROTOCOL.INI file are in the Advanced Settings
section.


     ***         ***         ***         ***          ***         ***


GENERAL NDIS 2.X DRIVER NOTES
=============================

Location of Driver:      \DOS\E100B.DOS
                         \OS2\E100B.OS2

Support files:           \DOS\E100BEDS.NIF
                         \OS2\E100BEO2.NIF
                         \DOS\OEMSETUP.INF
                         \DOS\PROTOCOL.INI

Sample Configuration Files
--------------------------

CONFIG.SYS (DOS version is similar to the following:)
   DEVICE=C:\path\PROTMAN.DOS /I:C:\path
   DEVICE=C:\path\E100B.DOS

CONFIG.SYS (OS/2* version is similar to the following:)
   DEVICE=C:\path\PROTMAN.OS2 /I:C:\path
   DEVICE=C:\path\E100B.OS2

PROTOCOL.INI (may contain)
   [PROTMAN]
   DriverName = PROTMAN$
   
   [NETBEUI_XIF]
   Drivername = netbeui$
   Sessions = 6
   NCBS = 12
   Bindings = "E100B_NIF"
   LANABASE = 0
   
   [E100B_NIF]
   Drivername = E100B$


General Notes
-------------

Several network operating systems use a standard 2.0.1 version NDIS
driver to talk to the network adapter. The adapter's NDIS driver
conforms to the Microsoft NDIS 2.0.1 specification.

The NDIS subdirectory on the Configuration and Drivers disk contains the 
files needed to use the adapter card with one of these operating
systems. The files and their purpose are listed below.

E100B.DOS:     NDIS driver for DOS workstations.

E100B.OS2:     NDIS driver for servers & OS/2 workstations.

E100BEDS.NIF:  The Extended Network Information file (NIF) that IBM LAN
               Support uses during its installation process. Specify the
               \DOS directory when installing so the installation
               procedure will find the correct NIF file.

E100BEO2.NIF:  The Extended Network Information file (NIF) that IBM OS/2
               uses during its installation process. Specify the \OS2
               directory when installing so the installation procedure
               will find the correct NIF file.

PROTOCOL.INI:  A fragment of the general PROTOCOL.INI file. This
               fragment contains information specific to the Intel
               adapter. Be sure your file contains this fragment. Some
               installation procedures create this file for you. This
               file is provided as an example of what the Intel 
               adapter section could look like.

OEMSETUP.INF:  The version located in the \DOS subdirectory on the
               driver disk is used by IBM's LAN requester for DOS
               version 4.0.


Hints and Tips
--------------

Parameters for the PROTOCOL.INI file are in the Advanced Settings
section.


     ***         ***         ***         ***          ***         ***


ADVANCED SETTINGS
=================

DRIVERNAME: (required) If you have a single adapter, use the syntax
      in the Sample Configuration File section.  If you are installing
      multiple adapters, each adapter must have a unique driver name.
      Additional instances of the driver would be referenced by
      DRIVERNAME=E100Bx$, where "x" is a unique number 2 through 9.
   
   SPEED: (optional; parameters are [Auto / 10 / 100]) The parameter
      disables Auto-Speed Detect and causes the adapter to function at
      the speed indicated. If the FORCEDUPLEX parameter is assigned to
      either 1 or 2, the SPEED parameter is required because auto-speed
      sensing is disabled if the duplex mode is forced. Auto-negotiate
      devices cannot detect speed changes in this configuration until
      the driver is reloaded. [Example: SPEED=100]
   
   FORCEDUPLEX: Full duplex and auto-negotiate capabilities vary between
      the PRO/100 TX and the PRO/100 T4 adapters.

         PRO/100+ TX adapter: Supports auto-negotiate, full
         and half duplex at 10 or 100 Mbps.

         PRO/100B T4 adapter: Supports full and half duplex
         at 10 Mbps; supports only half duplex at 100 Mbps.  Auto-
         negotiate is not a valid option at either speed.
   
      This parameter disables Auto-Negotiate capability and forces the
      adapter to operate in Half or Full Duplex mode. The SPEED 
      parameter must be specified and must be valid if the default of
      Auto-negotiate is changed. Options for FORCEDUPLEX are Auto (for
      auto-negotiate), 1 (for half), 2 (for full).
      [Example: FORCEDUPLEX = 2]
   
   SLOT: (required for multiple adapters) This parameter is optional if
      only one adapter is present.  If it is specified but is incorrect,
      a message indicates that the value doesn't match the configuration
      but the driver finds the adapter and loads anyway.
   
      This parameter is required if more than one adapter is present in
      either one bus or multiple PCI buses of a system. The parameter
      tells the driver which adapter it controls. The SLOT number is the
      encoded value of the PCI adapter's device location. To determine
      the slot number, load the driver with only the DRIVERNAME
      parameter specified.  The driver reports all the slots that have
      PCI adapter(s) installed. You can determine which card is in which
      slot by using SETUP.EXE and matching the Ethernet addresses of the
      adapter to the device number specified in View Configuration.
      [Example: SLOT=0x1C]
   
   NODE: (optional) This value sets the adapter's Individual Address,
      overriding the value read from the adapter EEprom. The address
      must consist of 12 hexadecimal digits, enclosed in double quotes.
      The value can not be all zeros. The value can not have the
      Multicast bit set. So, use only the hexadecimal digits 2, 6, A, or
      E as the second digit of the twelve required in the NODE ADDRESS
      parameter. Use any hexadecimal digits in all other positions.
      [Example: NODE ="02AA00123456"]



*  Third-party trademarks are the property of their respective owners.



