Windows NT4.0 Installation:

There are two methods to install sound driver:

(1) Auto installation:
1. Login Windows NT4.0

2. Insert the CD-ROM into the drive -enter the \PIM-582\SOUND\NT40
   directory on the CD-ROM and double-click SETUP.EXE.

3. Follow the prompts to complete the installation.

4. Restart your system.


(2) Manual installation:
1. Login Windows NT4.0

2. Open " My Computer ", and select " Control Panel " icon. 

3. Select " Multimedia " icon, and then select " Devices " page.

4. If you have other sound drivers installed, please remove them with 
   the " Remove " button and restart Windows NT before continuing. 
   
5. Click " Add... " button. 

6. Select " Unlisted or Updated Driver " selection bar, and then click " OK "
   button, an " Install Driver " window will appear. Please insert the CD
   Driver into the CD drive.

7. Type in " D:\PIM-582\SOUND\NT40 ", then click " OK " button.
   Note: D: is the drive where CD Driver has been inserted.

8. A " Add Unlisted or Updated Driver " windows appears. The line " 
   ESS AudioDrive ES1938/xx/xx/ Version x.x " will now be listed.

9. Press " OK " button.

10.Click " Restart Now " button to re-boot your computer.

