## Release Notes – 123Scan Scanner Configuration Utility v2.8

Introduction

Description

Contents

Device Compatibility

Installation Requirements

Installation Instructions

Part Number and Release Date

## Introduction

123Scan is an easy-to-use PC based application that will help you program your Motorola bar code scanning products.

- Allows easy scanner configuration
- Easy to create Advanced Data Formatting Rules
- Compatible with: Windows 2000 and XP

## Description

Addition of LS3578, DS3407DP, LS4208PDF & MS440xDP product support

## Contents

## 1. 123SCAN-00-2800.exe

## Device Compatibility

Definitions

- Printout means that you use 123Scan to generate a list of programming bar codes that can be scanned to program the scanner.
- Direct Connect means 123Scan can communicate with your scanner through an interface cable.

Listed below are the scanners supported by the 123Scan Scanner Configuration Utility.

# Scanner | # 123Scan Support
DS3407 | Printout;Direct Connect (RS232)
DS3407DP | Printout;Direct Connect (RS232)
DS3408 | Printout;Direct Connect (RS232)
DS3478 | Printout;Direct Connect (RS232) through cradle
DS6607 | Printout;Direct Connect (RS232)
DS6608 | Printout;Direct Connect (RS232)
DS6707 | Printout;Direct Connect (RS232)
DS6708 | Printout;Direct Connect (RS232)
LS1203 | Printout;Direct Connect (RS232)
LS1902 | Printout
LS1908 | Printout;Direct Connect (RS232)
LS2108 | Printout;Direct Connect (RS232)
LS2208 | Printout; Direct connect (RS232)
LS3008 | Printout;Direct Connect (RS232)
LS3408ER | Printout;Direct Connect (RS232)
LS3408FZY | Printout; Direct connect (RS232)
LS3478 | Printout; Direct connect (RS232) through cradle
LS3578 | Printout; Direct connect (RS232) through cradle
LS4008i | Printout; Direct connect (RS232)
LS4208 | Printout; Direct connect (RS232)
LS4208PDF | Printout; Direct connect (RS232)
LS4278 | Printout; Direct connect (RS232)
LS7708 | Printout; Direct connect (RS232) Note: When configuring the LS7708, an auxiliary scanner should not be connected. If you wish to program the auxiliary scanner, please use the 123Scan program directly for that scanner.
LS7808 | Printout; Direct connect (RS232) Note: When configuring the LS7808, an auxiliary scanner should not be connected. If you wish to program the auxiliary scanner, please use the 123Scan program directly for that scanner.
LS920x | Printout; Direct connect (RS232)
MS1207FZY | Printout;Direct Connect (RS232)
MS2207 | Printout;Direct Connect (RS232)
MS3207 | Printout;Direct Connect (RS232)
MS440xDP | Printout; Direct connect (RS232)
P304-I100 | Printout; Direct connect (RS232)
P360 | Printout;Direct Connect (RS232) Rev Q firmware or later
P460 | Printout; Direct connect (RS232) Rev Q firmware or later
P370 | Printout; Direct connect (RS232) Rev G firmware or later
P470 | Printout; Direct connect (RS232) Rev G firmware or later
PL4407 | Printout; Direct connect (RS232)

## Installation Requirements

- Windows 2000 or XP

## Installation Instructions

1. Download 123Scan InstallShield executable and save it to your computer
2. Run 123SCAN-00-2800.exe and follow the instructions.

## Part Number and Release Date

123SCAN-00-2800
September 2007